Beep Codes

|  |  |  |
| --- | --- | --- |
| **Beep signal**  | **Additional indicators**  | **Meaning** |
| continuous beep  |  | * System board failure
 |
| one beep  | unreadable, blank or flashing LCD  | * LCD connector problem
* LCD backlight inverter failure
* [video](http://www.thinkwiki.org/wiki/Error_Codes_and_Beep_Codes) adapter faulty
* LCD assembly faulty
* System board failure
* power supply failure
 |
| one beep  | Message "Unable to access boot source"  | * Boot device failure; system board failure
 |
| one long, two short beeps  |  | * System board failure
* Video adapter problem
* LCD assembly failure
 |
| one beep, three short beepsthree short beeps, one beep  |  | * Memory problem: bad DIMM or bad DIMM [slot](http://www.thinkwiki.org/wiki/Error_Codes_and_Beep_Codes)
 |
| one long, four short beeps  |  | * Low battery voltage
 |
| one beep every second  |  | * Low battery voltage
 |
| two short beeps  | error codes  | * [POST](http://www.thinkwiki.org/wiki/Error_Codes_and_Beep_Codes) error message
 |
| two short beeps  |  | * System board failure
 |